$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000009273, lin=000000000110, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '1005_(TY162)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'TSB1N15H2G45NS024T')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		ButtonProp('CircuitNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Application,Type,Case Size,Thickness,Passband,Passband (Low),Passband (Mid),Passband (High),Frequency Range\
;TSB1N15H2G45NS024T,Bluetooth/Wi-Fi/ZigBee,Band Pass Filter,1.0x0.5[mm],0.4[mm],2400MHz - 2500MHz,-,-,-,500MHz - 8.5GHz\
')
	$end 'Parameters'
$end '1005_(TY162)'
$begin '1608_(TY162)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'TSB1N18F2G45NS001T')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		ButtonProp('CircuitNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Application,Type,Case Size,Thickness,Passband,Passband (Low),Passband (Mid),Passband (High),Frequency Range\
;TSB1N18F2G45NS001T,Bluetooth/Wi-Fi/ZigBee,Band Pass Filter,1.6x0.8[mm],0.5[mm],2400MHz - 2500MHz,-,-,-,500MHz - 8.5GHz\
')
	$end 'Parameters'
$end '1608_(TY162)'
$begin '1608L_(TY162)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'TSB1N18D5G53LV0FWT')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		ButtonProp('CircuitNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Application,Type,Case Size,Thickness,Passband,Passband (Low),Passband (Mid),Passband (High),Frequency Range\
;TSB1N18D5G53LV0FWT,LTE(LAA)/Wi-Fi,Band Pass Filter,1.6x0.8[mm],0.65[mm],5150MHz - 5925MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N18D5G53LV0HBT,Wi-Fi,Band Pass Filter,1.6x0.8[mm],0.65[mm],5150MHz - 5925MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N18D845MLV0D9T,LTE-M/NB-IOT,Band Pass Filter,1.6x0.8[mm],0.65[mm],729MHz - 960MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N18D2G00LV0H7T,LTE-M/NB-IOT,Band Pass Filter,1.6x0.8[mm],0.65[mm],1805MHz - 2200MHz,-,-,-,50MHz - 15.05GHz\
')
	$end 'Parameters'
$end '1608L_(TY162)'
$begin '1608L2_(TY162)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'TSB1N18D7G24LV0K2T')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		ButtonProp('CircuitNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Application,Type,Case Size,Thickness,Passband,Passband (Low),Passband (Mid),Passband (High),Frequency Range\
;TSB1N18D7G24LV0K2T,UWB,Band Pass Filter,1.6x0.8[mm],0.65[mm],6240MHz - 8250MHz,-,-,-,500MHz - 16.5GHz\
;TSB1N18D3G75LV0KVT,5G,Band Pass Filter,1.6x0.8[mm],0.65[mm],3300MHz - 4200MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N18D4G70LV0KWT,5G,Band Pass Filter,1.6x0.8[mm],0.65[mm],4400MHz - 5000MHz,-,-,-,100MHz - 18.1GHz\
')
	$end 'Parameters'
$end '1608L2_(TY162)'
$begin '2012L_(TY162)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'TSB1N21D3G75LV0EQT')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		ButtonProp('CircuitNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 'nport:@ID %0 %1 0 0 np=2 file="$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p " dc=SO interp=Cubic', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 'S@ID %0 %1 0 FQMODEL=\\"@(Model)\\" Zo=50', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', '.model @(model) S TSTONEFILE=\\"$USERLIB/TaiyoYuden/_Sparameter/@(Model).s2p \\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Application,Type,Case Size,Thickness,Passband,Passband (Low),Passband (Mid),Passband (High),Frequency Range\
;TSB1N21D3G75LV0EQT,LTE/5G,Band Pass Filter,2.0x1.25[mm],0.65[mm],3300MHz - 4200MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N21D4G15LV0HWT,5G,Band Pass Filter,2.0x1.25[mm],0.65[mm],3300MHz - 5000MHz,-,-,-,100MHz - 18.1GHz\
;TSB1N21D4G70LV0DQT,5G,Band Pass Filter,2.0x1.25[mm],0.65[mm],4400MHz - 5000MHz,-,-,-,100MHz - 18.1GHz\
')
	$end 'Parameters'
$end '2012L_(TY162)'
$begin 'CompInfo'
	'1005_(TY162)'(4294901765, 2, 'Measured Data (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'bpf_TY', '', 'BPF_1005_S_TY', '', '', '', 'bbpf.bmp', 'TaiyoYuden\\Ceramic_RF_Device\\General_Equipment', 'UserLibrary ')
	'1608_(TY162)'(4294901765, 2, 'Measured Data (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'bpf_TY', '', 'BPF_1608_S_TY', '', '', '', 'bbpf.bmp', 'TaiyoYuden\\Ceramic_RF_Device\\General_Equipment', 'UserLibrary ')
	'1608L_(TY162)'(4294901765, 2, 'Measured Data (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'bpf_TY', '', 'BPF_1608L_S_TY', '', '', '', 'bbpf.bmp', 'TaiyoYuden\\Ceramic_RF_Device\\General_Equipment', 'UserLibrary ')
	'1608L2_(TY162)'(4294901765, 2, 'Measured Data (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'bpf_TY', '', 'BPF_1608L_S2_TY', '', '', '', 'bbpf.bmp', 'TaiyoYuden\\Ceramic_RF_Device\\General_Equipment', 'UserLibrary ')
	'2012L_(TY162)'(4294901765, 2, 'Measured Data (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'bpf_TY', '', 'BPF_2012L_S_TY', '', '', '', 'bbpf.bmp', 'TaiyoYuden\\Ceramic_RF_Device\\General_Equipment', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'1005_(TY162)'(pos=370, lin=11, lvl=0)
		'1608_(TY162)'(pos=1779, lin=28, lvl=0)
		'1608L_(TY162)'(pos=3188, lin=45, lvl=0)
		'1608L2_(TY162)'(pos=4923, lin=65, lvl=0)
		'2012L_(TY162)'(pos=6525, lin=84, lvl=0)
		CompInfo(pos=8131, lin=103, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=9273, lin=110, lvl=0)
	$end '$index$'
$end '$index$'
