$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000012142, lin=000000000164, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '2012_(TY037)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LSEUC2012HKTR47M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.2mm')
		VariableProp('A', 'RHD', '', '0.8mm')
		VariableProp('B', 'RHD', '', '0.6mm')
		VariableProp('C', 'RHD', '', '1.4mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LSEUC2012HKTR47M,0.47[uH],+/-20[%],2.0x1.2[mm],0.8[mm],4500[mA] (dL = 30[%]),3800[mA] (dT = 40[degC]),0.033[Ohm],-,100kHz - 208.503118MHz\
;LSEUC2012HKT1R0M,1[uH],+/-20[%],2.0x1.2[mm],0.8[mm],3200[mA] (dL = 30[%]),2300[mA] (dT = 40[degC]),0.078[Ohm],-,100kHz - 140.89697MHz\
;LSEUC2012KKTR33M,0.33[uH],+/-20[%],2.0x1.2[mm],1.0[mm],5800[mA] (dL = 30[%]),4600[mA] (dT = 40[degC]),0.024[Ohm],-,100kHz - 224.402193MHz\
;LSEUC2012KKTR47M,0.47[uH],+/-20[%],2.0x1.2[mm],1.0[mm],5000[mA] (dL = 30[%]),4300[mA] (dT = 40[degC]),0.027[Ohm],-,100kHz - 189.042664MHz\
;LSEUC2012MKTR11M,0.11[uH],+/-20[%],2.0x1.2[mm],1.2[mm],12000[mA] (dL = 30[%]),7500[mA] (dT = 40[degC]),0.0085[Ohm],-,100kHz - 375.343504MHz\
;LSEUC2012MKTR24M,0.24[uH],+/-20[%],2.0x1.2[mm],1.2[mm],8500[mA] (dL = 30[%]),5600[mA] (dT = 40[degC]),0.016[Ohm],-,100kHz - 247.502633MHz\
;LSEUC2012MKTR47M,0.47[uH],+/-20[%],2.0x1.2[mm],1.2[mm],4500[mA] (dL = 30[%]),4300[mA] (dT = 40[degC]),0.027[Ohm],-,100kHz - 175.64884MHz\
')
	$end 'Parameters'
$end '2012_(TY037)'
$begin '2016_(TY037)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LSEUC2016HKTR47M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '0.8mm')
		VariableProp('B', 'RHD', '', '0.6mm')
		VariableProp('C', 'RHD', '', '1.8mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LSEUC2016HKTR47M,0.47[uH],+/-20[%],2.0x1.6[mm],0.8[mm],4900[mA] (dL = 30[%]),4200[mA] (dT = 40[degC]),0.028[Ohm],-,100kHz - 159.254811MHz\
;LSEUC2016HKT1R0M,1[uH],+/-20[%],2.0x1.6[mm],0.8[mm],3200[mA] (dL = 30[%]),3000[mA] (dT = 40[degC]),0.05[Ohm],-,100kHz - 124.6553MHz\
;LSEUC2016KKTR47M,0.47[uH],+/-20[%],2.0x1.6[mm],1.0[mm],6300[mA] (dL = 30[%]),4700[mA] (dT = 40[degC]),0.026[Ohm],-,100kHz - 159.254811MHz\
;LSEUC2016KKT1R0M,1[uH],+/-20[%],2.0x1.6[mm],1.0[mm],4100[mA] (dL = 30[%]),3500[mA] (dT = 40[degC]),0.048[Ohm],-,100kHz - 121.638923MHz\
')
	$end 'Parameters'
$end '2016_(TY037)'
$begin '2520_(TY037)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LSEUC2520KKT1R0M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2.5mm')
		VariableProp('W', 'RHD', '', '2mm')
		VariableProp('A', 'RHD', '', '1mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '2.2mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LSEUC2520KKT1R0M,1[uH],+/-20[%],2.5x2.0[mm],1.0[mm],4400[mA] (dL = 30[%]),3600[mA] (dT = 40[degC]),0.037[Ohm],-,100kHz - 99.992428MHz\
;LSEUC2520KKT2R2M,2.2[uH],+/-20[%],2.5x2.0[mm],1.0[mm],3000[mA] (dL = 30[%]),2500[mA] (dT = 40[degC]),0.076[Ohm],-,100kHz - 78.268192MHz\
;LSEUC2520KKT4R7M,4.7[uH],+/-20[%],2.5x2.0[mm],1.0[mm],2200[mA] (dL = 30[%]),1800[mA] (dT = 40[degC]),0.16[Ohm],-,100kHz - 62.782943MHz\
;LSEUC2520KKT6R8M,6.8[uH],+/-20[%],2.5x2.0[mm],1.0[mm],1200[mA] (dL = 30[%]),1300[mA] (dT = 40[degC]),0.265[Ohm],-,100kHz - 56.923153MHz\
;LSEUC2520KKT100M,10[uH],+/-20[%],2.5x2.0[mm],1.0[mm],1000[mA] (dL = 30[%]),1000[mA] (dT = 40[degC]),0.432[Ohm],-,100kHz - 55.545741MHz\
')
	$end 'Parameters'
$end '2520_(TY037)'
$begin '3225_(TY037)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LSEUC3225HKT1R0M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '3.2mm')
		VariableProp('W', 'RHD', '', '2.5mm')
		VariableProp('A', 'RHD', '', '1.1mm')
		VariableProp('B', 'RHD', '', '1.3mm')
		VariableProp('C', 'RHD', '', '2.7mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LSEUC3225HKT1R0M,1[uH],+/-20[%],3.2x2.5[mm],0.8[mm],5200[mA] (dL = 30[%]),4200[mA] (dT = 40[degC]),0.043[Ohm],-,100kHz - 82.198079MHz\
')
	$end 'Parameters'
$end '3225_(TY037)'
$begin '4040_(TY037)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LSEUB4040WKTR47M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '4mm')
		VariableProp('W', 'RHD', '', '4mm')
		VariableProp('A', 'RHD', '', '1.7mm')
		VariableProp('B', 'RHD', '', '1.5mm')
		VariableProp('C', 'RHD', '', '4.3mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LSEUB4040WKTR47M,0.47[uH],+/-20[%],4.0x4.0[mm],2.0[mm],14000[mA] (dL = 30[%]),9900[mA] (dT = 40[degC]),0.0065[Ohm],-,100kHz - 78.268192MHz\
;LSEUB4040WKTR68M,0.68[uH],+/-20[%],4.0x4.0[mm],2.0[mm],11000[mA] (dL = 30[%]),8400[mA] (dT = 40[degC]),0.009[Ohm],-,100kHz - 64.339822MHz\
;LSEUB4040WKT1R0M,1[uH],+/-20[%],4.0x4.0[mm],2.0[mm],10000[mA] (dL = 30[%]),7700[mA] (dT = 40[degC]),0.0105[Ohm],-,100kHz - 54.20166MHz\
;LSEUB4040WKT2R2M,2.2[uH],+/-20[%],4.0x4.0[mm],2.0[mm],7000[mA] (dL = 30[%]),5300[mA] (dT = 40[degC]),0.021[Ohm],-,100kHz - 38.46609MHz\
')
	$end 'Parameters'
$end '4040_(TY037)'
$begin 'CompInfo'
	'2012_(TY037)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\General_Equipment', 'UserLibrary ')
	'2016_(TY037)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\General_Equipment', 'UserLibrary ')
	'2520_(TY037)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\General_Equipment', 'UserLibrary ')
	'3225_(TY037)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\General_Equipment', 'UserLibrary ')
	'4040_(TY037)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\General_Equipment', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'2012_(TY037)'(pos=370, lin=11, lvl=0)
		'2016_(TY037)'(pos=2901, lin=43, lvl=0)
		'2520_(TY037)'(pos=5006, lin=72, lvl=0)
		'3225_(TY037)'(pos=7244, lin=102, lvl=0)
		'4040_(TY037)'(pos=8936, lin=128, lvl=0)
		CompInfo(pos=11043, lin=157, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=12142, lin=164, lvl=0)
	$end '$index$'
$end '$index$'
