$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000009602, lin=000000000138, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '1608_(TY124)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLMCC160808T280NG')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1.6mm')
		VariableProp('W', 'RHD', '', '0.8mm')
		VariableProp('A', 'RHD', '', '1mm')
		VariableProp('B', 'RHD', '', '1mm')
		VariableProp('C', 'RHD', '', '1mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Impedance (100MHz),Tolerance (100MHz),Impedance (1GHz),Tolerance (1GHz),Case Size,Thickness,Rated Current,DC Resistance (MAX),Frequency Range\
;LLMCC160808T280NG,28[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],4[A],0.007[Ohm],1MHz - 3GHz\
;LLMCA160808T230NG,23[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],4[A],0.007[Ohm],1MHz - 3GHz\
;LLMCC160808T220NGR,22[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],7.5[A],0.004[Ohm],1MHz - 3GHz\
;LLMCC160808T280NGR,28[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],6[A],0.006[Ohm],1MHz - 3GHz\
;LLMCA160808T180NGR,18[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],7.5[A],0.004[Ohm],1MHz - 3GHz\
;LLMCA160808T230NGR,23[Ohm],+/-30[%],-,-,1.6x0.8[mm],0.8[mm],6[A],0.006[Ohm],1MHz - 3GHz\
')
	$end 'Parameters'
$end '1608_(TY124)'
$begin '2012_(TY124)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLMCC201208T250NG')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.25mm')
		VariableProp('A', 'RHD', '', '1.4mm')
		VariableProp('B', 'RHD', '', '1.2mm')
		VariableProp('C', 'RHD', '', '1.65mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Impedance (100MHz),Tolerance (100MHz),Impedance (1GHz),Tolerance (1GHz),Case Size,Thickness,Rated Current,DC Resistance (MAX),Frequency Range\
;LLMCC201208T250NG,25[Ohm],+/-30[%],-,-,2.0x1.25[mm],0.85[mm],6[A],0.004[Ohm],1MHz - 3GHz\
;LLMCC201208T420RG,42[Ohm],+/-25[%],-,-,2.0x1.25[mm],0.85[mm],4[A],0.008[Ohm],1MHz - 3GHz\
;LLMCA201208T210NG,21[Ohm],+/-30[%],-,-,2.0x1.25[mm],0.85[mm],6[A],0.004[Ohm],1MHz - 3GHz\
;LLMCA201208T330RG,33[Ohm],+/-25[%],-,-,2.0x1.25[mm],0.85[mm],4[A],0.008[Ohm],1MHz - 3GHz\
;LLMCG201208T8R0NG,8[Ohm],+/-30[%],-,-,2.0x1.25[mm],0.85[mm],4[A],0.008[Ohm],1MHz - 3GHz\
')
	$end 'Parameters'
$end '2012_(TY124)'
$begin '3216_(TY124)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLMCC321611T480NG')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '3.2mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '1.4mm')
		VariableProp('B', 'RHD', '', '2.2mm')
		VariableProp('C', 'RHD', '', '2mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Impedance (100MHz),Tolerance (100MHz),Impedance (1GHz),Tolerance (1GHz),Case Size,Thickness,Rated Current,DC Resistance (MAX),Frequency Range\
;LLMCC321611T480NG,48[Ohm],+/-30[%],-,-,3.2x1.6[mm],1.1[mm],6[A],0.005[Ohm],1MHz - 3GHz\
;LLMCC321611T800RG,80[Ohm],+/-25[%],-,-,3.2x1.6[mm],1.1[mm],4[A],0.01[Ohm],1MHz - 3GHz\
;LLMCA321611T380NG,38[Ohm],+/-30[%],-,-,3.2x1.6[mm],1.1[mm],6[A],0.005[Ohm],1MHz - 3GHz\
;LLMCA321611T600RG,60[Ohm],+/-25[%],-,-,3.2x1.6[mm],1.1[mm],4[A],0.01[Ohm],1MHz - 3GHz\
;LLMCG321611T160NG,16[Ohm],+/-30[%],-,-,3.2x1.6[mm],1.1[mm],4[A],0.012[Ohm],1MHz - 3GHz\
')
	$end 'Parameters'
$end '3216_(TY124)'
$begin '4516_(TY124)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLMCC451611T720NG')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '4.5mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '1.75mm')
		VariableProp('B', 'RHD', '', '3.5mm')
		VariableProp('C', 'RHD', '', '2mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Impedance (100MHz),Tolerance (100MHz),Impedance (1GHz),Tolerance (1GHz),Case Size,Thickness,Rated Current,DC Resistance (MAX),Frequency Range\
;LLMCC451611T720NG,72[Ohm],+/-30[%],-,-,4.5x1.6[mm],1.1[mm],6[A],0.007[Ohm],1MHz - 3GHz\
;LLMCC451611T111RG,110[Ohm],+/-25[%],-,-,4.5x1.6[mm],1.1[mm],4[A],0.014[Ohm],1MHz - 3GHz\
;LLMCA451611T560NG,56[Ohm],+/-30[%],-,-,4.5x1.6[mm],1.1[mm],6[A],0.007[Ohm],1MHz - 3GHz\
;LLMCA451611T900RG,90[Ohm],+/-25[%],-,-,4.5x1.6[mm],1.1[mm],4[A],0.014[Ohm],1MHz - 3GHz\
;LLMCG451611T230NG,23[Ohm],+/-30[%],-,-,4.5x1.6[mm],1.1[mm],3.5[A],0.014[Ohm],1MHz - 3GHz\
')
	$end 'Parameters'
$end '4516_(TY124)'
$begin 'CompInfo'
	'1608_(TY124)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Ferrite_Bead_Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'2012_(TY124)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Ferrite_Bead_Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'3216_(TY124)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Ferrite_Bead_Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'4516_(TY124)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Ferrite_Bead_Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'1608_(TY124)'(pos=370, lin=11, lvl=0)
		'2012_(TY124)'(pos=2489, lin=42, lvl=0)
		'3216_(TY124)'(pos=4526, lin=72, lvl=0)
		'4516_(TY124)'(pos=6550, lin=102, lvl=0)
		CompInfo(pos=8580, lin=132, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=9602, lin=138, lvl=0)
	$end '$index$'
$end '$index$'
