$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000010824, lin=000000000162, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '0402_(TY034)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MEASA042SB5224KWNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '0.4mm')
		VariableProp('W', 'RHD', '', '0.2mm')
		VariableProp('A', 'RHD', '', '0.15mm')
		VariableProp('B', 'RHD', '', '0.2mm')
		VariableProp('C', 'RHD', '', '0.2mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MEASA042SB5224KWNA01,0.22[uF],+/-10[%],0.4x0.2[mm],0.2[mm],4[V],X5R,10kHz - 3GHz\
;MEASA042SB5224MWNA01,0.22[uF],+/-20[%],0.4x0.2[mm],0.2[mm],4[V],X5R,10kHz - 3GHz\
;MEASA042SC6224MWNA01,0.22[uF],+/-20[%],0.4x0.2[mm],0.2[mm],4[V],X6S,10kHz - 3GHz\
;MEASP042SC6224MWNA01,0.22[uF],+/-20[%],0.4x0.2[mm],0.2[mm],2.5[V],X6S,10kHz - 3GHz\
')
	$end 'Parameters'
$end '0402_(TY034)'
$begin '0603_(TY034)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MEASA065QB5475MANC12')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '0.6mm')
		VariableProp('W', 'RHD', '', '0.3mm')
		VariableProp('A', 'RHD', '', '0.25mm')
		VariableProp('B', 'RHD', '', '0.3mm')
		VariableProp('C', 'RHD', '', '0.3mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MEASA065QB5475MANC12,4.7[uF],+/-20[%],0.6x0.3[mm],0.5[mm],4[V],X5R,1kHz - 3GHz\
;MEASA063BB5225MFNA01,2.2[uF],+/-20[%],0.6x0.3[mm],0.3[mm],4[V],X5R,1kHz - 3GHz\
;MEASA062PB5105MFNA01,1[uF],+/-20[%],0.6x0.3[mm],0.2[mm],4[V],X5R,1kHz - 3GHz\
;MEASJ065QC6225MANA01,2.2[uF],+/-20[%],0.6x0.3[mm],0.5[mm],6.3[V],X6S,1kHz - 3GHz\
;MEASP063BC6225MFNB46,2.2[uF],+/-20[%],0.6x0.3[mm],0.3[mm],2.5[V],X6S,1kHz - 3GHz\
;MEASP062PD6105MFNA01,1[uF],+/-20[%],0.6x0.3[mm],0.2[mm],2.5[V],X6T,1kHz - 3GHz\
')
	$end 'Parameters'
$end '0603_(TY034)'
$begin '1005_(TY034)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MEASL105BB5475KFNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1mm')
		VariableProp('W', 'RHD', '', '0.5mm')
		VariableProp('A', 'RHD', '', '0.4mm')
		VariableProp('B', 'RHD', '', '0.5mm')
		VariableProp('C', 'RHD', '', '0.5mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MEASL105BB5475KFNA01,4.7[uF],+/-10[%],1.0x0.5[mm],0.5[mm],10[V],X5R,1kHz - 3GHz\
;MEASL105BB5475MFNB33,4.7[uF],+/-20[%],1.0x0.5[mm],0.5[mm],10[V],X5R,1kHz - 3GHz\
;MEASJ105CB5106MFNC12,10[uF],+/-20[%],1.0x0.5[mm],0.5[mm],6.3[V],X5R,100Hz - 3GHz\
;MEASA105CB5226MFNC12,22[uF],+/-20[%],1.0x0.5[mm],0.5[mm],4[V],X5R,100Hz - 3GHz\
;MEASJ1L3NB5475MFNA01,4.7[uF],+/-20[%],1.0x0.5[mm],0.3[mm],6.3[V],X5R,1kHz - 3GHz\
;MEASA105NC6226MA1A01,22[uF],+/-20[%],1.0x0.5[mm],0.5[mm],4[V],X6S,100Hz - 3GHz\
;MEASP105CC6226MFNC12,22[uF],+/-20[%],1.0x0.5[mm],0.5[mm],2.5[V],X6S,100Hz - 3GHz\
')
	$end 'Parameters'
$end '1005_(TY034)'
$begin '1608_(TY034)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MEASA168BB5476MT1A01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1.6mm')
		VariableProp('W', 'RHD', '', '0.8mm')
		VariableProp('A', 'RHD', '', '0.6mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '0.8mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MEASA168BB5476MT1A01,47[uF],+/-20[%],1.6x0.8[mm],0.8[mm],4[V],X5R,100Hz - 3GHz\
')
	$end 'Parameters'
$end '1608_(TY034)'
$begin '2012_(TY034)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MEASA21GBB5107MTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.25mm')
		VariableProp('A', 'RHD', '', '0.8mm')
		VariableProp('B', 'RHD', '', '1mm')
		VariableProp('C', 'RHD', '', '1.25mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MEASA21GBB5107MTNA01,100[uF],+/-20[%],2.0x1.25[mm],1.25[mm],4[V],X5R,100Hz - 3GHz\
')
	$end 'Parameters'
$end '2012_(TY034)'
$begin 'CompInfo'
	'0402_(TY034)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Only_for_Mobile_devices', 'UserLibrary ')
	'0603_(TY034)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Only_for_Mobile_devices', 'UserLibrary ')
	'1005_(TY034)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Only_for_Mobile_devices', 'UserLibrary ')
	'1608_(TY034)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Only_for_Mobile_devices', 'UserLibrary ')
	'2012_(TY034)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Only_for_Mobile_devices', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'0402_(TY034)'(pos=370, lin=11, lvl=0)
		'0603_(TY034)'(pos=2249, lin=40, lvl=0)
		'1005_(TY034)'(pos=4282, lin=71, lvl=0)
		'1608_(TY034)'(pos=6399, lin=103, lvl=0)
		'2012_(TY034)'(pos=8024, lin=129, lvl=0)
		CompInfo(pos=9650, lin=155, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=10824, lin=162, lvl=0)
	$end '$index$'
$end '$index$'
