$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000009100, lin=000000000137, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '1608_(TY005)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MSAYU168BLD224KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1.6mm')
		VariableProp('W', 'RHD', '', '0.8mm')
		VariableProp('A', 'RHD', '', '0.6mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '0.8mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MSAYU168BLD224KTNA01,0.22[uF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],X5R,10kHz - 3GHz\
;MSAYU168BLD224MTNA01,0.22[uF],+/-20[%],1.6x0.8[mm],0.8[mm],50[V],X5R,10kHz - 3GHz\
;MSAYT168BLD474KTNA01,0.47[uF],+/-10[%],1.6x0.8[mm],0.8[mm],25[V],X5R,10kHz - 3GHz\
;MSAYT168BLD474MTNA01,0.47[uF],+/-20[%],1.6x0.8[mm],0.8[mm],25[V],X5R,10kHz - 3GHz\
;MSAYT168BLD105KTNA01,1[uF],+/-10[%],1.6x0.8[mm],0.8[mm],25[V],X5R,1kHz - 3GHz\
;MSAYT168BLD105MTNA01,1[uF],+/-20[%],1.6x0.8[mm],0.8[mm],25[V],X5R,1kHz - 3GHz\
')
	$end 'Parameters'
$end '1608_(TY005)'
$begin '2012_(TY005)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MSAYG21GSLD105KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.25mm')
		VariableProp('A', 'RHD', '', '0.8mm')
		VariableProp('B', 'RHD', '', '1mm')
		VariableProp('C', 'RHD', '', '1.25mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MSAYG21GSLD105KTNA01,1[uF],+/-10[%],2.0x1.25[mm],1.25[mm],35[V],X5R,1kHz - 3GHz\
;MSAYG21GSLD105MTNA01,1[uF],+/-20[%],2.0x1.25[mm],1.25[mm],35[V],X5R,1kHz - 3GHz\
;MSAYG21GBLD225KTNA01,2.2[uF],+/-10[%],2.0x1.25[mm],1.25[mm],35[V],X5R,1kHz - 3GHz\
;MSAYG21GBLD225MTNA01,2.2[uF],+/-20[%],2.0x1.25[mm],1.25[mm],35[V],X5R,1kHz - 3GHz\
')
	$end 'Parameters'
$end '2012_(TY005)'
$begin '3216_(TY005)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MSAYU31LSLD105KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '3.2mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '1mm')
		VariableProp('B', 'RHD', '', '2.2mm')
		VariableProp('C', 'RHD', '', '1.6mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MSAYU31LSLD105KTNA01,1[uF],+/-10[%],3.2x1.6[mm],1.6[mm],50[V],X5R,1kHz - 3GHz\
;MSAYU31LSLD105MTNA01,1[uF],+/-20[%],3.2x1.6[mm],1.6[mm],50[V],X5R,1kHz - 3GHz\
;MSAYG31LBLD475KTNA01,4.7[uF],+/-10[%],3.2x1.6[mm],1.6[mm],35[V],X5R,1kHz - 3GHz\
;MSAYG31LBLD475MTNA01,4.7[uF],+/-20[%],3.2x1.6[mm],1.6[mm],35[V],X5R,1kHz - 3GHz\
;MSAYT31LBLD106KTNA01,10[uF],+/-10[%],3.2x1.6[mm],1.6[mm],25[V],X5R,100Hz - 3GHz\
;MSAYT31LBLD106MTNA01,10[uF],+/-20[%],3.2x1.6[mm],1.6[mm],25[V],X5R,100Hz - 3GHz\
')
	$end 'Parameters'
$end '3216_(TY005)'
$begin '3225_(TY005)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MSAYU32MSLD475KPNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '3.2mm')
		VariableProp('W', 'RHD', '', '2.5mm')
		VariableProp('A', 'RHD', '', '1mm')
		VariableProp('B', 'RHD', '', '2mm')
		VariableProp('C', 'RHD', '', '2.5mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MSAYU32MSLD475KPNA01,4.7[uF],+/-10[%],3.2x2.5[mm],2.5[mm],50[V],X5R,1kHz - 3GHz\
;MSAYU32MSLD475MPNA01,4.7[uF],+/-20[%],3.2x2.5[mm],2.5[mm],50[V],X5R,1kHz - 3GHz\
;MSAYU32NSLD105KTNA01,1[uF],+/-10[%],3.2x2.5[mm],1.9[mm],50[V],X5R,1kHz - 3GHz\
;MSAYU32NSLD105MTNA01,1[uF],+/-20[%],3.2x2.5[mm],1.9[mm],50[V],X5R,1kHz - 3GHz\
')
	$end 'Parameters'
$end '3225_(TY005)'
$begin 'CompInfo'
	'1608_(TY005)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\General_Equipment', 'UserLibrary ')
	'2012_(TY005)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\General_Equipment', 'UserLibrary ')
	'3216_(TY005)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\General_Equipment', 'UserLibrary ')
	'3225_(TY005)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\General_Equipment', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'1608_(TY005)'(pos=370, lin=11, lvl=0)
		'2012_(TY005)'(pos=2410, lin=42, lvl=0)
		'3216_(TY005)'(pos=4284, lin=71, lvl=0)
		'3225_(TY005)'(pos=6314, lin=102, lvl=0)
		CompInfo(pos=8178, lin=131, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=9100, lin=137, lvl=0)
	$end '$index$'
$end '$index$'
