$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000006596, lin=000000000097, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '2012_(TY096)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLEPC2012HKTR47M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.2mm')
		VariableProp('A', 'RHD', '', '0.7mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '1.4mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LLEPC2012HKTR47M,0.47[uH],+/-20[%],2.0x1.2[mm],0.8[mm],4100[mA] (dL = 30[%]),3700[mA] (dT = 40[degC]),0.035[Ohm],-,100kHz - 213.673535MHz\
;LLEPC2012KKTR47M,0.47[uH],+/-20[%],2.0x1.2[mm],1.0[mm],4500[mA] (dL = 30[%]),4200[mA] (dT = 40[degC]),0.03[Ohm],-,100kHz - 203.457813MHz\
')
	$end 'Parameters'
$end '2012_(TY096)'
$begin '2016_(TY096)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLEPC2016KKTR47M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '0.7mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '1.8mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LLEPC2016KKTR47M,0.47[uH],+/-20[%],2.0x1.6[mm],1.0[mm],5300[mA] (dL = 30[%]),4700[mA] (dT = 40[degC]),0.026[Ohm],-,100kHz - 193.730505MHz\
;LLEPC2016KKT1R0M,1[uH],+/-20[%],2.0x1.6[mm],1.0[mm],4000[mA] (dL = 30[%]),3500[mA] (dT = 40[degC]),0.048[Ohm],-,100kHz - 137.487582MHz\
;LLEPC2016KKT2R2M,2.2[uH],+/-20[%],2.0x1.6[mm],1.0[mm],2300[mA] (dL = 30[%]),2300[mA] (dT = 40[degC]),0.1[Ohm],-,100kHz - 110.285862MHz\
')
	$end 'Parameters'
$end '2016_(TY096)'
$begin '2520_(TY096)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'LLEPC2520KKT1R0M')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2.5mm')
		VariableProp('W', 'RHD', '', '2mm')
		VariableProp('A', 'RHD', '', '0.9mm')
		VariableProp('B', 'RHD', '', '1mm')
		VariableProp('C', 'RHD', '', '2.2mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Inductance,Tolerance,Case Size,Thickness,Rated Current,Rated Current2,DC Resistance (MAX),SRF (MIN),Frequency Range\
;LLEPC2520KKT1R0M,1[uH],+/-20[%],2.5x2.0[mm],1.0[mm],4400[mA] (dL = 30[%]),3800[mA] (dT = 40[degC]),0.039[Ohm],-,100kHz - 118.695536MHz\
')
	$end 'Parameters'
$end '2520_(TY096)'
$begin 'CompInfo'
	'2012_(TY096)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'2016_(TY096)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'2520_(TY096)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'indv_TY', '', 'FootPrint_TY', '', '', '', 'ind.bmp', 'TaiyoYuden\\Inductor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'2012_(TY096)'(pos=370, lin=11, lvl=0)
		'2016_(TY096)'(pos=2203, lin=38, lvl=0)
		'2520_(TY096)'(pos=4171, lin=66, lvl=0)
		CompInfo(pos=5860, lin=92, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=6596, lin=97, lvl=0)
	$end '$index$'
$end '$index$'
