$begin '$base_index$'
  $begin 'properties'
    all_levels=000000000000
    time(year=000000002025, month=000000000011, day=000000000012, hour=000000000013, min=000000000010, sec=000000000036)
    version=000000000000
  $end 'properties'
  $begin '$base_index$'
    $index$(pos=000000011969, lin=000000000171, lvl=000000000000)
  $end '$base_index$'
$end '$base_index$'
$begin '1005_(TY030)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MLAYU105SSD391KFNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1mm')
		VariableProp('W', 'RHD', '', '0.5mm')
		VariableProp('A', 'RHD', '', '0.4mm')
		VariableProp('B', 'RHD', '', '0.5mm')
		VariableProp('C', 'RHD', '', '0.5mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MLAYU105SSD391KFNA01,390[pF],+/-10[%],1.0x0.5[mm],0.5[mm],50[V],-,40Hz - 3GHz\
;MLAYU105SSD471KFNA01,470[pF],+/-10[%],1.0x0.5[mm],0.5[mm],50[V],-,40Hz - 3GHz\
;MLAYU105SSD561KFNA01,560[pF],+/-10[%],1.0x0.5[mm],0.5[mm],50[V],-,40Hz - 3GHz\
;MLAYT105SSD681KFNA01,680[pF],+/-10[%],1.0x0.5[mm],0.5[mm],25[V],-,40Hz - 3GHz\
;MLAYT105SSD821KFNA01,820[pF],+/-10[%],1.0x0.5[mm],0.5[mm],25[V],-,40Hz - 3GHz\
;MLAYT105SSD102KFNA01,1000[pF],+/-10[%],1.0x0.5[mm],0.5[mm],25[V],-,40Hz - 3GHz\
;MLAYT105SSD122KFNA01,1200[pF],+/-10[%],1.0x0.5[mm],0.5[mm],25[V],-,40Hz - 3GHz\
;MLAYE105SSD152KFNA01,1500[pF],+/-10[%],1.0x0.5[mm],0.5[mm],16[V],-,40Hz - 3GHz\
;MLAYE105SSD182KFNA01,1800[pF],+/-10[%],1.0x0.5[mm],0.5[mm],16[V],-,40Hz - 3GHz\
;MLAYE105SSD222KFNA01,2200[pF],+/-10[%],1.0x0.5[mm],0.5[mm],16[V],-,40Hz - 3GHz\
;MLAYE105SSD272KFNA01,2700[pF],+/-10[%],1.0x0.5[mm],0.5[mm],16[V],-,40Hz - 3GHz\
;MLAYL105SSD332KFNA01,3300[pF],+/-10[%],1.0x0.5[mm],0.5[mm],10[V],-,40Hz - 3GHz\
;MLAYL105SSD392KFNA01,3900[pF],+/-10[%],1.0x0.5[mm],0.5[mm],10[V],-,40Hz - 3GHz\
;MLAYL105SSD472KFNA01,4700[pF],+/-10[%],1.0x0.5[mm],0.5[mm],10[V],-,40Hz - 3GHz\
')
	$end 'Parameters'
$end '1005_(TY030)'
$begin '1608_(TY030)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MLAYU168SSD102KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '1.6mm')
		VariableProp('W', 'RHD', '', '0.8mm')
		VariableProp('A', 'RHD', '', '0.6mm')
		VariableProp('B', 'RHD', '', '0.8mm')
		VariableProp('C', 'RHD', '', '0.8mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MLAYU168SSD102KTNA01,1000[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD122KTNA01,1200[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD152KTNA01,1500[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD182KTNA01,1800[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD222KTNA01,2200[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD272KTNA01,2700[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYU168SSD332KTNA01,3300[pF],+/-10[%],1.6x0.8[mm],0.8[mm],50[V],-,40Hz - 3GHz\
;MLAYT168SSD392KTNA01,3900[pF],+/-10[%],1.6x0.8[mm],0.8[mm],25[V],-,40Hz - 3GHz\
;MLAYT168SSD472KTNA01,4700[pF],+/-10[%],1.6x0.8[mm],0.8[mm],25[V],-,40Hz - 3GHz\
;MLAYE168SSD562KTNA01,5600[pF],+/-10[%],1.6x0.8[mm],0.8[mm],16[V],-,40Hz - 3GHz\
;MLAYE168SSD682KTNA01,6800[pF],+/-10[%],1.6x0.8[mm],0.8[mm],16[V],-,40Hz - 3GHz\
;MLAYE168SSD822KTNA01,8200[pF],+/-10[%],1.6x0.8[mm],0.8[mm],16[V],-,40Hz - 3GHz\
;MLAYE168SSD103KTNA01,0.01[uF],+/-10[%],1.6x0.8[mm],0.8[mm],16[V],-,40Hz - 3GHz\
;MLAYL168SSD123KTNA01,0.012[uF],+/-10[%],1.6x0.8[mm],0.8[mm],10[V],-,40Hz - 3GHz\
;MLAYL168SSD153KTNA01,0.015[uF],+/-10[%],1.6x0.8[mm],0.8[mm],10[V],-,40Hz - 3GHz\
;MLAYL168SSD183KTNA01,0.018[uF],+/-10[%],1.6x0.8[mm],0.8[mm],10[V],-,40Hz - 3GHz\
;MLAYL168SSD223KTNA01,0.022[uF],+/-10[%],1.6x0.8[mm],0.8[mm],10[V],-,40Hz - 3GHz\
')
	$end 'Parameters'
$end '1608_(TY030)'
$begin '2012_(TY030)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MLAYG21GSSD183KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '2mm')
		VariableProp('W', 'RHD', '', '1.25mm')
		VariableProp('A', 'RHD', '', '0.8mm')
		VariableProp('B', 'RHD', '', '1mm')
		VariableProp('C', 'RHD', '', '1.25mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MLAYG21GSSD183KTNA01,0.018[uF],+/-10[%],2.0x1.25[mm],1.25[mm],35[V],-,40Hz - 3GHz\
;MLAYG21GSSD223KTNA01,0.022[uF],+/-10[%],2.0x1.25[mm],1.25[mm],35[V],-,40Hz - 3GHz\
;MLAYG21GSSD273KTNA01,0.027[uF],+/-10[%],2.0x1.25[mm],1.25[mm],35[V],-,40Hz - 3GHz\
;MLAYL21GSSD683KTNA01,0.068[uF],+/-10[%],2.0x1.25[mm],1.25[mm],10[V],-,40Hz - 3GHz\
;MLAYL21GSSD823KTNA01,0.082[uF],+/-10[%],2.0x1.25[mm],1.25[mm],10[V],-,40Hz - 3GHz\
;MLAYL21GSSD104KTNA01,0.1[uF],+/-10[%],2.0x1.25[mm],1.25[mm],10[V],-,40Hz - 3GHz\
;MLAYU219SSD392KTNA01,3900[pF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYU219SSD472KTNA01,4700[pF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYU219SSD562KTNA01,5600[pF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYU219SSD682KTNA01,6800[pF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYU219SSD822KTNA01,8200[pF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYU219SSD103KTNA01,0.01[uF],+/-10[%],2.0x1.25[mm],0.85[mm],50[V],-,40Hz - 3GHz\
;MLAYG219SSD123KTNA01,0.012[uF],+/-10[%],2.0x1.25[mm],0.85[mm],35[V],-,40Hz - 3GHz\
;MLAYG219SSD153KTNA01,0.015[uF],+/-10[%],2.0x1.25[mm],0.85[mm],35[V],-,40Hz - 3GHz\
;MLAYE219SSD333KTNA01,0.033[uF],+/-10[%],2.0x1.25[mm],0.85[mm],16[V],-,40Hz - 3GHz\
;MLAYL219SSD473KTNA01,0.047[uF],+/-10[%],2.0x1.25[mm],0.85[mm],10[V],-,40Hz - 3GHz\
')
	$end 'Parameters'
$end '2012_(TY030)'
$begin '3216_(TY030)'
	Refbase='X'
	NumParts=1
	Terminal('1', '1', 'A', false, 0, 0, 0)
	Terminal('2', '2', 'A', false, 1, 0, 0)
	$begin 'Parameters'
		TextProp('Model', 'RD', '', 'MLAYT31LSSD823KTNA01')
		ButtonProp('VComp', 'OID', '', 'Choose Model', '', 0)
		TextProp('DeviceLibraryName', 'RHD', '', 'TaiyoYuden.lib')
		TextProp('NexximLibraryName', 'RHD', '', 'Nexxim_TaiyoYuden.lib')
		VariableProp('L', 'RHD', '', '3.2mm')
		VariableProp('W', 'RHD', '', '1.6mm')
		VariableProp('A', 'RHD', '', '1mm')
		VariableProp('B', 'RHD', '', '2.2mm')
		VariableProp('C', 'RHD', '', '1.6mm')
		ButtonProp('CircuitNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('SystemNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('NexximNetList', 'RHD', '', 'X@ID %0 %1 @Model', 'X@ID %0 %1 @Model', 1)
		ButtonProp('CircuitGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('SystemGlobalRef', 'RHD', '', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', '.lib \\"$USERLIB/TaiyoYuden/_Netlist/@DeviceLibraryName\\"', 1)
		ButtonProp('NexximGlobalRef', 'RHD', '', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', '.inc \\"$USERLIB/TaiyoYuden/_Netlist/@NexximLibraryName\\"', 1)
		TextProp('ModelList', 'RHD', '', 'Model,Capacitance,Tolerance,Case Size,Thickness,Rated Voltage,Temperature Characteristics,Frequency Range\
;MLAYT31LSSD823KTNA01,0.082[uF],+/-10[%],3.2x1.6[mm],1.6[mm],25[V],-,40Hz - 3GHz\
;MLAYT31LSSD104KTNA01,0.1[uF],+/-10[%],3.2x1.6[mm],1.6[mm],25[V],-,40Hz - 3GHz\
;MLAYG31QHSD333KTNA01,0.033[uF],+/-10[%],3.2x1.6[mm],1.15[mm],35[V],-,40Hz - 3GHz\
;MLAYG31QHSD393KTNA01,0.039[uF],+/-10[%],3.2x1.6[mm],1.15[mm],35[V],-,40Hz - 3GHz\
;MLAYT31QHSD473KTNA01,0.047[uF],+/-10[%],3.2x1.6[mm],1.15[mm],25[V],-,40Hz - 3GHz\
;MLAYT31QHSD563KTNA01,0.056[uF],+/-10[%],3.2x1.6[mm],1.15[mm],25[V],-,40Hz - 3GHz\
;MLAYT31QHSD683KTNA01,0.068[uF],+/-10[%],3.2x1.6[mm],1.15[mm],25[V],-,40Hz - 3GHz\
')
	$end 'Parameters'
$end '3216_(TY030)'
$begin 'CompInfo'
	'1005_(TY030)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'1608_(TY030)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'2012_(TY030)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
	'3216_(TY030)'(4294901765, 2, 'Equivalent Model (All Rights Reserved)', 1762920636, 'Taiyo Yuden', 'capv_TY', '', 'FootPrint_TY', '', '', '', 'cap.bmp', 'TaiyoYuden\\Ceramic_Capacitor\\Medical_(International_Class_I_and_II)', 'UserLibrary ')
$end 'CompInfo'
$begin '$index$'
	$begin '$index$'
		'1005_(TY030)'(pos=370, lin=11, lvl=0)
		'1608_(TY030)'(pos=3041, lin=50, lvl=0)
		'2012_(TY030)'(pos=5966, lin=92, lvl=0)
		'3216_(TY030)'(pos=8844, lin=133, lvl=0)
		CompInfo(pos=10963, lin=165, lvl=0)
		$base_index$(pos=0, lin=1, lvl=0)
		$index$(pos=11969, lin=171, lvl=0)
	$end '$index$'
$end '$index$'
